{
    "board_id": 9,
    "magic": "APJFWv1",
    "description": "Firmware for a STM32F427xx board",
    "image": "[encoded data, 900556 characters]",
    "extf_image": "eNoDAAAAAAE=",
    "summary": "Pixhawk1-1M",
    "version": "0.1",
    "image_size": 980464,
    "extf_image_size": 0,
    "flash_total": 1032192,
    "image_maxsize": 1032192,
    "flash_free": 51728,
    "extflash_total": 0,
    "extflash_free": 0,
    "git_identity": "960ca66d",
    "board_revision": 0,
    "USBID": "0x1209/0x5741"
}